# `ggswissmaps` data with `sf`

#### gibo

#### 2025-06-23

From version `0.1.2`, `ggswissmaps` includes boundaries of Switzerland, at various levels, also in `sf` format. The 8 objects are stored in the list `shp_sf`:

    library(ggswissmaps)
    # str(shp_sf)  # Very long output...

    class(shp_sf)
    #> [1] "list"
    length(shp_sf)
    #> [1] 8
    lapply(shp_sf, class)
    #> $g1b15
    #> [1] "sf"         "data.frame"
    #>
    #> $g1g15_encl
    #> [1] "sf"         "data.frame"
    #>
    #> $g1g15_li
    #> [1] "sf"         "data.frame"
    #>
    #> $g1g15
    #> [1] "sf"         "data.frame"
    #>
    #> $g1k15
    #> [1] "sf"         "data.frame"
    #>
    #> $g1l15
    #> [1] "sf"         "data.frame"
    #>
    #> $g1r15
    #> [1] "sf"         "data.frame"
    #>
    #> $g1s15
    #> [1] "sf"         "data.frame"
    names(shp_sf)
    #> [1] "g1b15"      "g1g15_encl" "g1g15_li"   "g1g15"      "g1k15"
    #> [6] "g1l15"      "g1r15"      "g1s15"

# Use `ggswissmaps` with `sf`

The boundaries stored in the list `shp_sf` can be used with `ggplot2::geom_sf()`:

    library(ggplot2)
    ggplot(shp_sf[["g1k15"]]) + geom_sf()
    #> old-style crs object detected; please recreate object with a recent sf::st_crs()
    #> old-style crs object detected; please recreate object with a recent sf::st_crs()
    #> old-style crs object detected; please recreate object with a recent sf::st_crs()

The gray background can be removed for example with `ggswissmaps::theme_white_f()` or other `ggplot2` themes, while the gray background inside the boundaries can be removed by setting `fill = NA` in `ggplot2::geom_sf()`:

    ggplot(shp_sf[["g1k15"]]) +
      geom_sf(fill = NA) +
      ggswissmaps::theme_white_f()
    #> old-style crs object detected; please recreate object with a recent sf::st_crs()
    #> old-style crs object detected; please recreate object with a recent sf::st_crs()
    #> old-style crs object detected; please recreate object with a recent sf::st_crs()

# Coordinate reference system (crs)

Note that all the ‘sf’ data frames stored in the list `shp_sf` have the coordinate reference system (crs) corrensponding to “EPSG: 21781”. This can be verified with `sf::st_crs()`:

    library(sf)
    #> Linking to GEOS 3.13.1, GDAL 3.11.0, PROJ 9.6.0; sf_use_s2() is TRUE
    st_crs(shp_sf[[1]])
    #> old-style crs object detected; please recreate object with a recent sf::st_crs()
    #> Coordinate Reference System:
    #>   User input: EPSG:21781
    #>   wkt:
    #> PROJCRS["CH1903 / LV03",
    #>     BASEGEOGCRS["CH1903",
    #>         DATUM["CH1903",
    #>             ELLIPSOID["Bessel 1841",6377397.155,299.1528128,
    #>                 LENGTHUNIT["metre",1]]],
    #>         PRIMEM["Greenwich",0,
    #>             ANGLEUNIT["degree",0.0174532925199433]],
    #>         ID["EPSG",4149]],
    #>     CONVERSION["Swiss Oblique Mercator 1903M",
    #>         METHOD["Hotine Oblique Mercator (variant B)",
    #>             ID["EPSG",9815]],
    #>         PARAMETER["Latitude of projection centre",46.9524055555556,
    #>             ANGLEUNIT["degree",0.0174532925199433],
    #>             ID["EPSG",8811]],
    #>         PARAMETER["Longitude of projection centre",7.43958333333333,
    #>             ANGLEUNIT["degree",0.0174532925199433],
    #>             ID["EPSG",8812]],
    #>         PARAMETER["Azimuth at projection centre",90,
    #>             ANGLEUNIT["degree",0.0174532925199433],
    #>             ID["EPSG",8813]],
    #>         PARAMETER["Angle from Rectified to Skew Grid",90,
    #>             ANGLEUNIT["degree",0.0174532925199433],
    #>             ID["EPSG",8814]],
    #>         PARAMETER["Scale factor at projection centre",1,
    #>             SCALEUNIT["unity",1],
    #>             ID["EPSG",8815]],
    #>         PARAMETER["Easting at projection centre",600000,
    #>             LENGTHUNIT["metre",1],
    #>             ID["EPSG",8816]],
    #>         PARAMETER["Northing at projection centre",200000,
    #>             LENGTHUNIT["metre",1],
    #>             ID["EPSG",8817]]],
    #>     CS[Cartesian,2],
    #>         AXIS["easting (Y)",east,
    #>             ORDER[1],
    #>             LENGTHUNIT["metre",1]],
    #>         AXIS["northing (X)",north,
    #>             ORDER[2],
    #>             LENGTHUNIT["metre",1]],
    #>     USAGE[
    #>         SCOPE["Cadastre, engineering survey, topographic mapping (large and medium scale)."],
    #>         AREA["Liechtenstein; Switzerland."],
    #>         BBOX[45.82,5.96,47.81,10.49]],
    #>     ID["EPSG",21781]]

I think that this is the “old” swiss crs, while the newest one is “EPSG: 2056”. In order to change the crs we can use `st::st_transform()`:

    tmp <- st_transform(shp_sf[[1]], crs = 2056)
    #> old-style crs object detected; please recreate object with a recent sf::st_crs()
    st_crs(tmp)
    #> Coordinate Reference System:
    #>   User input: EPSG:2056
    #>   wkt:
    #> PROJCRS["CH1903+ / LV95",
    #>     BASEGEOGCRS["CH1903+",
    #>         DATUM["CH1903+",
    #>             ELLIPSOID["Bessel 1841",6377397.155,299.1528128,
    #>                 LENGTHUNIT["metre",1]]],
    #>         PRIMEM["Greenwich",0,
    #>             ANGLEUNIT["degree",0.0174532925199433]],
    #>         ID["EPSG",4150]],
    #>     CONVERSION["Swiss Oblique Mercator 1995",
    #>         METHOD["Hotine Oblique Mercator (variant B)",
    #>             ID["EPSG",9815]],
    #>         PARAMETER["Latitude of projection centre",46.9524055555556,
    #>             ANGLEUNIT["degree",0.0174532925199433],
    #>             ID["EPSG",8811]],
    #>         PARAMETER["Longitude of projection centre",7.43958333333333,
    #>             ANGLEUNIT["degree",0.0174532925199433],
    #>             ID["EPSG",8812]],
    #>         PARAMETER["Azimuth at projection centre",90,
    #>             ANGLEUNIT["degree",0.0174532925199433],
    #>             ID["EPSG",8813]],
    #>         PARAMETER["Angle from Rectified to Skew Grid",90,
    #>             ANGLEUNIT["degree",0.0174532925199433],
    #>             ID["EPSG",8814]],
    #>         PARAMETER["Scale factor at projection centre",1,
    #>             SCALEUNIT["unity",1],
    #>             ID["EPSG",8815]],
    #>         PARAMETER["Easting at projection centre",2600000,
    #>             LENGTHUNIT["metre",1],
    #>             ID["EPSG",8816]],
    #>         PARAMETER["Northing at projection centre",1200000,
    #>             LENGTHUNIT["metre",1],
    #>             ID["EPSG",8817]]],
    #>     CS[Cartesian,2],
    #>         AXIS["(E)",east,
    #>             ORDER[1],
    #>             LENGTHUNIT["metre",1]],
    #>         AXIS["(N)",north,
    #>             ORDER[2],
    #>             LENGTHUNIT["metre",1]],
    #>     USAGE[
    #>         SCOPE["Cadastre, engineering survey, topographic mapping (large and medium scale)."],
    #>         AREA["Liechtenstein; Switzerland."],
    #>         BBOX[45.82,5.96,47.81,10.49]],
    #>     ID["EPSG",2056]]