<refentry id="vidioc-g-std">
  <refmeta>
    <refentrytitle>ioctl VIDIOC_G_STD, VIDIOC_S_STD</refentrytitle>
    &manvol;
  </refmeta>

  <refnamediv>
    <refname>VIDIOC_G_STD</refname>
    <refname>VIDIOC_S_STD</refname>
    <refpurpose>Query or select the video standard of the current input</refpurpose>
  </refnamediv>

  <refsynopsisdiv>
    <funcsynopsis>
      <funcprototype>
	<funcdef>int <function>ioctl</function></funcdef>
	<paramdef>int <parameter>fd</parameter></paramdef>
	<paramdef>int <parameter>request</parameter></paramdef>
	<paramdef>v4l2_std_id
*<parameter>argp</parameter></paramdef>
      </funcprototype>
    </funcsynopsis>
    <funcsynopsis>
      <funcprototype>
	<funcdef>int <function>ioctl</function></funcdef>
	<paramdef>int <parameter>fd</parameter></paramdef>
	<paramdef>int <parameter>request</parameter></paramdef>
	<paramdef>const v4l2_std_id
*<parameter>argp</parameter></paramdef>
      </funcprototype>
    </funcsynopsis>
  </refsynopsisdiv>

  <refsect1>
    <title>Arguments</title>

    <variablelist>
      <varlistentry>
	<term><parameter>fd</parameter></term>
	<listitem>
	  <para>&fd;</para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><parameter>request</parameter></term>
	<listitem>
	  <para>VIDIOC_G_STD, VIDIOC_S_STD</para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><parameter>argp</parameter></term>
	<listitem>
	  <para></para>
	</listitem>
      </varlistentry>
    </variablelist>
  </refsect1>

  <refsect1>
    <title>Description</title>

    <para>To query and select the current video standard applications
use the <constant>VIDIOC_G_STD</constant> and <constant>VIDIOC_S_STD</constant> ioctls which take a pointer to a
&v4l2-std-id; type as argument. <constant>VIDIOC_G_STD</constant> can
return a single flag or a set of flags as in &v4l2-standard; field
<structfield>id</structfield>. The flags must be unambiguous such
that they appear in only one enumerated <structname>v4l2_standard</structname> structure.</para>

    <para><constant>VIDIOC_S_STD</constant> accepts one or more
flags, being a write-only ioctl it does not return the actual new standard as
<constant>VIDIOC_G_STD</constant> does. When no flags are given or
the current input does not support the requested standard the driver
returns an &EINVAL;. When the standard set is ambiguous drivers may
return <errorcode>EINVAL</errorcode> or choose any of the requested
standards.</para>
  </refsect1>

  <refsect1>
    &return-value;

    <variablelist>
      <varlistentry>
	<term><errorcode>EINVAL</errorcode></term>
	<listitem>
	  <para>This ioctl is not supported, or the
<constant>VIDIOC_S_STD</constant> parameter was unsuitable.</para>
	</listitem>
      </varlistentry>
    </variablelist>
  </refsect1>
</refentry>

<!--
Local Variables:
mode: sgml
sgml-parent-document: "v4l2.sgml"
indent-tabs-mode: nil
End:
-->
