The LLVM Lexicon

NOTE: This document is a work in progress!

Table Of Contents

- A -
ADCE
- B -
BURS
- C -
CSE
- D -
DAG | Derived Pointer | DSA | DSE
- G -
| GC
- I -
IPA | IPO | ISel
- L -
LCSSA | LICM | Load-VN
- O -
Object Pointer
- P -
PRE
- R -
Reassociation | Root
- S -
Safe Point | SCC | SCCP | SDISel | SRoA | Stack Map

Definitions
- A -

ADCE
  Aggressive Dead Code Elimination

- B -

BURS
  Bottom Up Rewriting System - A method of instruction selection for code generation. An example is the BURG tool.

- C -

CSE
  Common Subexpression Elimination. An optimization that removes common subexpression compuation. For example `(a+b)*(a+b)` has two subexpressions that are the same: `(a+b)`. This optimization would perform the addition only once and then perform the multiply (but only if it's compulationally correct/safe).

- D -

DAG
  Directed Acyclic Graph
Derived Pointer
  A pointer to the interior of an object, such that a garbage collector is unable to use the pointer for reachability analysis. While a derived pointer is live, the corresponding object pointer must be kept in a root, otherwise the collector might free the referenced object. With copying collectors, derived pointers pose an additional hazard that they may be invalidated at any safe point. This term is used in opposition to object pointer.
DSA
  Data Structure Analysis
DSE
  Dead Store Elimination

- G -

GC
  Garbage Collection. The practice of using reachability analysis instead of explicit memory management to reclaim unused memory.

- H -

Heap
  In garbage collection, the region of memory which is managed using reachability analysis.

- I -

IPA
  Inter-Procedural Analysis. Refers to any variety of code analysis that occurs between procedures, functions or compilation units (modules).
IPO
  Inter-Procedural Optimization. Refers to any variety of code optimization that occurs between procedures, functions or compilation units (modules).
ISel
  Instruction Selection.

- L -

LCSSA
  Loop-Closed Static Single Assignment Form
LICM
  Loop Invariant Code Motion
Load-VN
  Load Value Numbering

- O -

Object Pointer
  A pointer to an object such that the garbage collector is able to trace references contained within the object. This term is used in opposition to derived pointer.

- P -

PRE
  Partial Redundancy Elimination

- R -

Reassociation
  Rearranging associative expressions to promote better redundancy elimination and other optimization. For example, changing (A+B-A) into (B+A-A), permitting it to be optimized into (B+0) then (B).
Root
  In garbage collection, a pointer variable lying outside of the heap from which the collector begins its reachability analysis. In the context of code generation, "root" almost always refers to a "stack root"—a local or temporary variable within an executing function.

- S -

Safe Point
  In garbage collection, it is necessary to identify stack roots so that reachability analysis may proceed. It may be infeasible to provide this information for every instruction, so instead the information may is calculated only at designated safe points. With a copying collector, derived pointers must not be retained across safe points and object pointers must be reloaded from stack roots.
SDISel
  Selection DAG Instruction Selection.
SCC
  Strongly Connected Component
SCCP
  Sparse Conditional Constant Propagation
SRoA
  Scalar Replacement of Aggregates
SSA
  Static Single Assignment
Stack Map
  In garbage collection, metadata emitted by the code generator which identifies roots within the stack frame of an executing function.