<<<
[#insns-c_lhu,reftext="c.lhu: Load unsigned halfword, 16-bit encoding"]
=== c.lhu

Synopsis::
Load unsigned halfword, 16-bit encoding

Mnemonic::
c.lhu _rd'_, _uimm_(_rs1'_)

Encoding (RV32, RV64)::
[wavedrom, , svg]
....
{reg:[
    { bits:  2, name: 0x0, attr: ['C0'] },
    { bits:  3, name: 'rd\'' },
    { bits:  1, name: 'uimm[1]' },
    { bits:  1, name: 0x0 },
    { bits:  3, name: 'rs1\'' },
    { bits:  3, name: 0x1 },
    { bits:  3, name: 0x4, attr: ['FUNCT3'] },
],config:{bits:16}}
....

include::c_lhsh_imm_offset.adoc[]

Description::
This instruction loads a halfword from the memory address formed by adding _rs1'_ to the zero extended immediate _uimm_. The resulting halfword is zero extended to XLEN bits and is written to _rd'_. 

[NOTE]
  _rd'_ and _rs1'_ are from the standard 8-register set x8-x15.

[NOTE]
  For an longer immediate with a 16-bit encoding see <<insns-cm_lhu>>.

Prerequisites::
None

32-bit equivalent::
<<insns-lhu>>

Operation::
[source,sail]
--
//This is not SAIL, it's pseudo-code. The SAIL hasn't been written yet.

X(rdc) = EXTZ(load_mem[X(rs1c)+EXTZ(uimm)][15..0]);
--

include::Zcb_footer.adoc[]

