<<<
[#insns-cm_mva01s,reftext="Move two s0-s7 registers into a0-a1"]
=== cm.mva01s

Synopsis::
Move two s0-s7 registers into a0-a1

Mnemonic::
cm.mva01s _sreg1_, _sreg2_

Encoding (RV32, RV64)::
[wavedrom, , svg]
....
{reg:[
    { bits:  2, name: 0x2,      attr: ['C2'] },
    { bits:  3, name: 'sreg2',  attr: [] },
    { bits:  2, name: 0x3,      attr: [] },
    { bits:  3, name: 'sreg1',  attr: [] },
    { bits:  3, name: 0x3,      attr: [] },
    { bits:  3, name: 0x5,      attr: ['FUNCT3'] },
],config:{bits:16}}
....

Assembly Syntax::

[source,sail]
--
cm.mva01s sreg1, sreg2
--

Description::
This instruction moves _sreg1_ into _a0_ and _sreg2_ into _a1_. 
The execution is atomic, so it is not possible to observe state where only one of _a0_ or _a1_ have been updated.

The encoding uses _sreg_ number specifiers instead of _xreg_ number specifiers to save encoding space. 
The mapping between them is specified in the pseudo-code below.

[NOTE]

  The _s_ register mapping is taken from the UABI, and may not match the currently unratified EABI. _cm.mva01s.e_ may be included in the future.

Prerequisites::
None

32-bit equivalent::
No direct equivalent encoding exists.

Operation::
[source,sail]
--
//This is not SAIL, it's pseudo-code. The SAIL hasn't been written yet.
if (RV32E && (sreg1>1 || sreg2>1)) {
  reserved();
}
xreg1 = {sreg1[2:1]>0,sreg1[2:1]==0,sreg1[2:0]};
xreg2 = {sreg2[2:1]>0,sreg2[2:1]==0,sreg2[2:0]};
X[10] = X[xreg1];
X[11] = X[xreg2];
--

include::Zcmp_footer.adoc[]

