- SeaBIOS (bios.bin) is the successor of pc bios.
  See http://www.seabios.org/ for more information.

- The VGA BIOS and the Cirrus VGA BIOS come from the LGPL VGA bios
  project (http://www.nongnu.org/vgabios/).

- The PowerPC Open Hack'Ware Open Firmware Compatible BIOS is
  available at http://perso.magic.fr/l_indien/OpenHackWare/index.htm.

- OpenBIOS (http://www.openbios.org/) is a free (GPL v2) portable
  firmware implementation. The goal is to implement a 100% IEEE
  1275-1994 (referred to as Open Firmware) compliant firmware.
  The included images for PowerPC (for 32 and 64 bit PPC CPUs),
  Sparc32 and Sparc64 are built from OpenBIOS SVN revision
  1060.

- SLOF (Slimline Open Firmware) is a free IEEE 1275 Open Firmware
  implementation for certain IBM POWER hardware.  The sources are at
  https://github.com/dgibson/SLOF, and the image currently in qemu is
  built from git tag qemu-slof-20120217.

- sgabios (the Serial Graphics Adapter option ROM) provides a means for
  legacy x86 software to communicate with an attached serial console as
  if a video card were attached.  The master sources reside in a subversion
  repository at http://sgabios.googlecode.com/svn/trunk.  A git mirror is
  available at git://git.qemu.org/sgabios.git.

- The PXE roms come from the iPXE project. Built with BANNER_TIME 0.
  Sources available at http://ipxe.org.  Vendor:Device ID -> ROM mapping:

	8086:100e -> pxe-e1000.rom
	8086:1209 -> pxe-eepro100.rom
	1050:0940 -> pxe-ne2k_pci.rom
	1022:2000 -> pxe-pcnet.rom
	10ec:8139 -> pxe-rtl8139.rom
	1af4:1000 -> pxe-virtio.rom

- The S390 zipl loader is an addition to the official IBM s390-tools
  package. That fork is maintained in its own git repository at:
  git://repo.or.cz/s390-tools.git

- The sources for the Alpha palcode image is available from:
  git://repo.or.cz/qemu-palcode.git
