From 69ef87e2bc8b929b7af75c3f03aafd1f12121b67 Mon Sep 17 00:00:00 2001
From: Aldy Hernandez <aldyh@gcc.gnu.org>
Date: Tue, 19 Feb 2002 02:53:41 +0000
Subject: i386.md ("mmx_uavgv8qi3"): Use const_vector.

2002-02-19  Aldy Hernandez  <aldyh@redhat.com>

	* config/i386/i386.md ("mmx_uavgv8qi3"): Use const_vector.
	("mmx_uavgv4hi3"): Same.
	("pmulhrwv4hi3"): Same.

	* tree-inline.c (walk_tree): Handle vectors.

	* c-common.c (constant_expression_warning): Handle vectors.
	(overflow_warning): Same.

	* sched-deps.c (sched_analyze_2): Handle vectors.

	* rtlanal.c (rtx_unstable_p): Handle vectors.
	(rtx_varies_p): Same.
	(count_occurrences): Same.
	(regs_set_between_p): Same.
	(modified_between_p): Same.
	(modified_in_p): Same.
	(volatile_insn_p): Same.
	(volatile_refs_p): Same.
	(side_effects_p): Same.
	(may_trap_p): Same.
	(inequality_comparisons_p): Same.
	(replace_regs): Same.
	(computed_jump_p_1): Same.

	* rtl.c (DEF_MACHMODE): Change all definitions to accept 8th
	argument.
	(inner_mode_array): New.
	(copy_rtx): Handle vectors.
	(copy_most_rtx): Same.
	(rtx_equal_p): Same.
	(get_mode_alignment): Adjust for vectors.

	* resource.c (mark_referenced_resources): Handle vectors.
	(mark_set_resources): Same.

	* reload1.c (eliminate_regs): Handle vectors.
	(elimination_effects): Same.
	(scan_paradoxical_subregs): Same.

	* reload.c (subst_reg_equivs): Handle vectors.

	* regrename.c (scan_rtx): Handle vectors.

	* regclass.c (reg_scan_mark_refs): Handle vectors.

	* recog.c (find_single_use_1): Handle vectors.

	* local-alloc.c (equiv_init_varies_p): Handle vectors.
	(contains_replace_regs): Same.
	(memref_referenced_p): Same.

	* integrate.c (copy_rtx_and_substitute): Handle vectors.
	(subst_constants): Same.

	* genattrtab.c (attr_copy_rtx): Handle vectors.
	(encode_units_mask): Same.
	(clear_struct_flag): Same.
	(count_sub_rtxs): Same.

	* gcse.c (want_to_gcse_p): Handle vectors.
	(oprs_unchanged_p): Same.
	(hash_expr_1): Same.
	(oprs_not_set_p): Same.
	(expr_killed_p): Same.
	(compute_transp): Same.
	(store_ops_ok): Same.

	* function.c (purge_addressof_1): Do not allow paradoxical subregs
	of vectors.
	(fixup_var_refs_1): Same.
	(instantiate_virtual_regs_1): Same.

	* fold-const.c (operand_equal_p): Handle vectors.
	(fold): Same.
	(rtl_expr_nonnegative_p): Same.

	* flow.c (mark_used_regs): Handle vectors.

	* df.c (df_uses_record): Handle vectors.

	* cselib.c (cselib_subst_to_values): Handle vectors.
	(cselib_mem_conflict_p): Same.
	(hash_rtx): Same.

	* cse.c (canon_reg): Handle vectors.
	(fold_rt): Same.
	(cse_process_notes): Same.
	(count_reg_usage): Same.
	(canon_hash): Same.

	* alias.c (nonlocal_mentioned_p): Add case for CONST_VECTOR.

	* combine.c (mark_used_regs_combine): Add case for CONST_VECTOR.

	* emit-rtl.c (init_emit_once): Generate const0_rtx for vectors.
	(gen_rtx): Handle CONST_VECTOR.
	(gen_const_vector_0): New.
	(copy_rtx_if_shared): CONST_VECTORs can be shared.
	(reset_used_flags): Same.
	(copy_insn_1): Same.
	(initializer_constant_valid_p): Handle VECTOR_CST.

	* doc/c-tree.texi (Expression trees): Document VECTOR_CST.

	* doc/rtl.texi (Constants): Document const_vector.
	(CONST0_RTX): Update for vectors.
	(RTL sharing): Same.

	* print-tree.c (print_node): Add case for VECTOR_CST.

	* tree.h (TREE_VECTOR_CST_ELTS): New.
	(struct tree_vector): New.
	(union tree_node): Add vector node.
	(build_vector): Add prototype.

	* tree.def (VECTOR_CST): New.

	* tree.c (build_vector): New.

	* expmed.c (make_tree): Handle CONST_VECTOR.

	* rtl.h (CONSTANT_P): CONST_VECTORs are constants too.
	(CONST_VECTOR_ELT): New.
	(CONST_VECTOR_NUNITS): New.

	* machmode.h (GET_MODE_INNER): New.
	(DEF_MACHMODE): Accept 8th arg.

	* machmode.def: Add 8th argument for vector inner mode.
	Add inner vector modes for vectors.

	* rtl.def (VEC_CONST): Remove.
	(CONST_VECTOR): New.

	* expr.c (clear_storage): Allow vectors.
	(is_zeros_p): Handle VECTOR_CST.

	* varasm.c (output_constant_pool): Handle vectors.
	(rtx_const): Add veclo and vechi fields.
	(kind): Add RTX_VECTOR.
	(decode_rtx_const): Add case for vector.

	* config/rs6000/rs6000-protos.h: Add zero_constant.

	* config/rs6000/rs6000.c (rs6000_emit_move): Handle vector
	constants.  Force easy vector constants into memory.
	(easy_vector_constant): New.
	(emit_easy_vector_constant): New.
	(rs6000_legitimize_reload_address): Do not generate bad reloads on
	darwin.

	* config/rs6000/rs6000.md ("altivec_lvx"): Reflect what
	instruction does.
	("altivec_lvxl"): Same.
	(altivec_lvebx): Same.
	(altivec_lvehx): Same.
	(altivec_lvewx): Same.
	("*movv4si_const0"): New.
	("*movv4sf_const0"): New.
	("*movv8hi_const0"): New.
	("*movv16qi_const0"): New.

From-SVN: r49853
---
 gcc/machmode.def | 118 ++++++++++++++++++++++++++++---------------------------
 1 file changed, 61 insertions(+), 57 deletions(-)

(limited to 'gcc/machmode.def')

diff --git a/gcc/machmode.def b/gcc/machmode.def
index 5ec6a1e..16abebb 100644
--- a/gcc/machmode.def
+++ b/gcc/machmode.def
@@ -63,50 +63,54 @@ Software Foundation, 59 Temple Place - Suite 330, Boston, MA
    there is none.  Vector modes use this field to point to the next
    vector size, so we can iterate through the different vectors modes.
    The ordering is by increasing byte size, with QI coming before HI,
-   HI before SI, etc.  */
+   HI before SI, etc.
+
+   Eigth arg is the mode of the internal elements in a vector.
+   VOIDmode if not a vector.
+*/
 
 /* VOIDmode is used when no mode needs to be specified,
    as for example on CONST_INT RTL expressions.  */
-DEF_MACHMODE (VOIDmode, "VOID", MODE_RANDOM, 0, 0, 0, VOIDmode)
+DEF_MACHMODE (VOIDmode, "VOID", MODE_RANDOM, 0, 0, 0, VOIDmode, VOIDmode)
 
-DEF_MACHMODE (BImode, "BI", MODE_INT, 1, 1, 1, QImode)
-DEF_MACHMODE (QImode, "QI", MODE_INT, BITS_PER_UNIT, 1, 1, HImode)
-DEF_MACHMODE (HImode, "HI", MODE_INT, BITS_PER_UNIT*2, 2, 2, SImode)
-DEF_MACHMODE (SImode, "SI", MODE_INT, BITS_PER_UNIT*4, 4, 4, DImode)
-DEF_MACHMODE (DImode, "DI", MODE_INT, BITS_PER_UNIT*8, 8, 8, TImode)
-DEF_MACHMODE (TImode, "TI", MODE_INT, BITS_PER_UNIT*16, 16, 16, OImode)
-DEF_MACHMODE (OImode, "OI", MODE_INT, BITS_PER_UNIT*32, 32, 32, VOIDmode)
+DEF_MACHMODE (BImode, "BI", MODE_INT, 1, 1, 1, QImode, VOIDmode)
+DEF_MACHMODE (QImode, "QI", MODE_INT, BITS_PER_UNIT, 1, 1, HImode, VOIDmode)
+DEF_MACHMODE (HImode, "HI", MODE_INT, BITS_PER_UNIT*2, 2, 2, SImode, VOIDmode)
+DEF_MACHMODE (SImode, "SI", MODE_INT, BITS_PER_UNIT*4, 4, 4, DImode, VOIDmode)
+DEF_MACHMODE (DImode, "DI", MODE_INT, BITS_PER_UNIT*8, 8, 8, TImode, VOIDmode)
+DEF_MACHMODE (TImode, "TI", MODE_INT, BITS_PER_UNIT*16, 16, 16, OImode, VOIDmode)
+DEF_MACHMODE (OImode, "OI", MODE_INT, BITS_PER_UNIT*32, 32, 32, VOIDmode, VOIDmode)
 
 /* Pointers on some machines use these types to distinguish them from
    ints.  Useful if a pointer is 4 bytes but has some bits that are
    not significant, so it is really not quite as wide as an integer.  */
-DEF_MACHMODE (PQImode, "PQI", MODE_PARTIAL_INT, BITS_PER_UNIT, 1, 1, PHImode)
-DEF_MACHMODE (PHImode, "PHI", MODE_PARTIAL_INT, BITS_PER_UNIT*2, 2, 2, PSImode)
-DEF_MACHMODE (PSImode, "PSI", MODE_PARTIAL_INT, BITS_PER_UNIT*4, 4, 4, PDImode)
-DEF_MACHMODE (PDImode, "PDI", MODE_PARTIAL_INT, BITS_PER_UNIT*8, 8, 8, VOIDmode)
-
-DEF_MACHMODE (QFmode, "QF", MODE_FLOAT, BITS_PER_UNIT, 1, 1, HFmode)
-DEF_MACHMODE (HFmode, "HF", MODE_FLOAT, BITS_PER_UNIT*2, 2, 2, TQFmode)
-DEF_MACHMODE (TQFmode, "TQF", MODE_FLOAT, BITS_PER_UNIT*3, 3, 3, SFmode) /* MIL-STD-1750A */
-DEF_MACHMODE (SFmode, "SF", MODE_FLOAT, BITS_PER_UNIT*4, 4, 4, DFmode)
-DEF_MACHMODE (DFmode, "DF", MODE_FLOAT, BITS_PER_UNIT*8, 8, 8, XFmode)
-DEF_MACHMODE (XFmode, "XF", MODE_FLOAT, BITS_PER_UNIT*12, 12, 12, TFmode) /* IEEE extended */
-DEF_MACHMODE (TFmode, "TF", MODE_FLOAT, BITS_PER_UNIT*16, 16, 16, VOIDmode)
+DEF_MACHMODE (PQImode, "PQI", MODE_PARTIAL_INT, BITS_PER_UNIT, 1, 1, PHImode, VOIDmode)
+DEF_MACHMODE (PHImode, "PHI", MODE_PARTIAL_INT, BITS_PER_UNIT*2, 2, 2, PSImode, VOIDmode)
+DEF_MACHMODE (PSImode, "PSI", MODE_PARTIAL_INT, BITS_PER_UNIT*4, 4, 4, PDImode, VOIDmode)
+DEF_MACHMODE (PDImode, "PDI", MODE_PARTIAL_INT, BITS_PER_UNIT*8, 8, 8, VOIDmode, VOIDmode)
+
+DEF_MACHMODE (QFmode, "QF", MODE_FLOAT, BITS_PER_UNIT, 1, 1, HFmode, VOIDmode)
+DEF_MACHMODE (HFmode, "HF", MODE_FLOAT, BITS_PER_UNIT*2, 2, 2, TQFmode, VOIDmode)
+DEF_MACHMODE (TQFmode, "TQF", MODE_FLOAT, BITS_PER_UNIT*3, 3, 3, SFmode, VOIDmode) /* MIL-STD-1750A */
+DEF_MACHMODE (SFmode, "SF", MODE_FLOAT, BITS_PER_UNIT*4, 4, 4, DFmode, VOIDmode)
+DEF_MACHMODE (DFmode, "DF", MODE_FLOAT, BITS_PER_UNIT*8, 8, 8, XFmode, VOIDmode)
+DEF_MACHMODE (XFmode, "XF", MODE_FLOAT, BITS_PER_UNIT*12, 12, 12, TFmode, VOIDmode) /* IEEE extended */
+DEF_MACHMODE (TFmode, "TF", MODE_FLOAT, BITS_PER_UNIT*16, 16, 16, VOIDmode, VOIDmode)
 
 /* Complex modes.  */
-DEF_MACHMODE (QCmode, "QC", MODE_COMPLEX_FLOAT, BITS_PER_UNIT*2, 2, 1, HCmode)
-DEF_MACHMODE (HCmode, "HC", MODE_COMPLEX_FLOAT, BITS_PER_UNIT*4, 4, 2, SCmode)
-DEF_MACHMODE (SCmode, "SC", MODE_COMPLEX_FLOAT, BITS_PER_UNIT*8, 8, 4, DCmode)
-DEF_MACHMODE (DCmode, "DC", MODE_COMPLEX_FLOAT, BITS_PER_UNIT*16, 16, 8, XCmode)
-DEF_MACHMODE (XCmode, "XC", MODE_COMPLEX_FLOAT, BITS_PER_UNIT*24, 24, 12, TCmode)
-DEF_MACHMODE (TCmode, "TC", MODE_COMPLEX_FLOAT, BITS_PER_UNIT*32, 32, 16, VOIDmode)
-
-DEF_MACHMODE (CQImode, "CQI", MODE_COMPLEX_INT, BITS_PER_UNIT*2, 2, 1, CHImode)
-DEF_MACHMODE (CHImode, "CHI", MODE_COMPLEX_INT, BITS_PER_UNIT*4, 4, 2, CSImode)
-DEF_MACHMODE (CSImode, "CSI", MODE_COMPLEX_INT, BITS_PER_UNIT*8, 8, 4, CDImode)
-DEF_MACHMODE (CDImode, "CDI", MODE_COMPLEX_INT, BITS_PER_UNIT*16, 16, 8, CTImode)
-DEF_MACHMODE (CTImode, "CTI", MODE_COMPLEX_INT, BITS_PER_UNIT*32, 32, 16, COImode)
-DEF_MACHMODE (COImode, "COI", MODE_COMPLEX_INT, BITS_PER_UNIT*64, 64, 32, VOIDmode)
+DEF_MACHMODE (QCmode, "QC", MODE_COMPLEX_FLOAT, BITS_PER_UNIT*2, 2, 1, HCmode, VOIDmode)
+DEF_MACHMODE (HCmode, "HC", MODE_COMPLEX_FLOAT, BITS_PER_UNIT*4, 4, 2, SCmode, VOIDmode)
+DEF_MACHMODE (SCmode, "SC", MODE_COMPLEX_FLOAT, BITS_PER_UNIT*8, 8, 4, DCmode, VOIDmode)
+DEF_MACHMODE (DCmode, "DC", MODE_COMPLEX_FLOAT, BITS_PER_UNIT*16, 16, 8, XCmode, VOIDmode)
+DEF_MACHMODE (XCmode, "XC", MODE_COMPLEX_FLOAT, BITS_PER_UNIT*24, 24, 12, TCmode, VOIDmode)
+DEF_MACHMODE (TCmode, "TC", MODE_COMPLEX_FLOAT, BITS_PER_UNIT*32, 32, 16, VOIDmode, VOIDmode)
+
+DEF_MACHMODE (CQImode, "CQI", MODE_COMPLEX_INT, BITS_PER_UNIT*2, 2, 1, CHImode, VOIDmode)
+DEF_MACHMODE (CHImode, "CHI", MODE_COMPLEX_INT, BITS_PER_UNIT*4, 4, 2, CSImode, VOIDmode)
+DEF_MACHMODE (CSImode, "CSI", MODE_COMPLEX_INT, BITS_PER_UNIT*8, 8, 4, CDImode, VOIDmode)
+DEF_MACHMODE (CDImode, "CDI", MODE_COMPLEX_INT, BITS_PER_UNIT*16, 16, 8, CTImode, VOIDmode)
+DEF_MACHMODE (CTImode, "CTI", MODE_COMPLEX_INT, BITS_PER_UNIT*32, 32, 16, COImode, VOIDmode)
+DEF_MACHMODE (COImode, "COI", MODE_COMPLEX_INT, BITS_PER_UNIT*64, 64, 32, VOIDmode, VOIDmode)
 
 /* Vector modes.  */
 /* There are no V1xx vector modes.  These are equivalent to normal
@@ -114,43 +118,43 @@ DEF_MACHMODE (COImode, "COI", MODE_COMPLEX_INT, BITS_PER_UNIT*64, 64, 32, VOIDmo
 /* The wider mode field for vectors follows in order of increasing bit
    size with QI coming before HI, HI before SI, and SI before DI
    within same bit sizes.  */
-DEF_MACHMODE (V2QImode, "V2QI", MODE_VECTOR_INT, BITS_PER_UNIT*2, 2, 1, V4QImode)
-DEF_MACHMODE (V2HImode, "V2HI", MODE_VECTOR_INT, BITS_PER_UNIT*4, 4, 2, V8QImode)
-DEF_MACHMODE (V2SImode, "V2SI", MODE_VECTOR_INT, BITS_PER_UNIT*8, 8, 4, V16QImode)
-DEF_MACHMODE (V2DImode, "V2DI", MODE_VECTOR_INT, BITS_PER_UNIT*16, 16, 8, V8SImode)
+DEF_MACHMODE (V2QImode, "V2QI", MODE_VECTOR_INT, BITS_PER_UNIT*2, 2, 1, V4QImode, QImode)
+DEF_MACHMODE (V2HImode, "V2HI", MODE_VECTOR_INT, BITS_PER_UNIT*4, 4, 2, V8QImode, HImode)
+DEF_MACHMODE (V2SImode, "V2SI", MODE_VECTOR_INT, BITS_PER_UNIT*8, 8, 4, V16QImode, SImode)
+DEF_MACHMODE (V2DImode, "V2DI", MODE_VECTOR_INT, BITS_PER_UNIT*16, 16, 8, V8SImode, DImode)
 
-DEF_MACHMODE (V4QImode, "V4QI", MODE_VECTOR_INT, BITS_PER_UNIT*4, 4, 1, V2HImode)
-DEF_MACHMODE (V4HImode, "V4HI", MODE_VECTOR_INT, BITS_PER_UNIT*8, 8, 2, V2SImode)
-DEF_MACHMODE (V4SImode, "V4SI", MODE_VECTOR_INT, BITS_PER_UNIT*16, 16, 4, V2DImode)
-DEF_MACHMODE (V4DImode, "V4DI", MODE_VECTOR_INT, BITS_PER_UNIT*32, 32, 8, V8DImode)
+DEF_MACHMODE (V4QImode, "V4QI", MODE_VECTOR_INT, BITS_PER_UNIT*4, 4, 1, V2HImode, QImode)
+DEF_MACHMODE (V4HImode, "V4HI", MODE_VECTOR_INT, BITS_PER_UNIT*8, 8, 2, V2SImode, HImode)
+DEF_MACHMODE (V4SImode, "V4SI", MODE_VECTOR_INT, BITS_PER_UNIT*16, 16, 4, V2DImode, SImode)
+DEF_MACHMODE (V4DImode, "V4DI", MODE_VECTOR_INT, BITS_PER_UNIT*32, 32, 8, V8DImode, DImode)
 
-DEF_MACHMODE (V8QImode, "V8QI", MODE_VECTOR_INT, BITS_PER_UNIT*8, 8, 1, V4HImode)
-DEF_MACHMODE (V8HImode, "V8HI", MODE_VECTOR_INT, BITS_PER_UNIT*16, 16, 2, V4SImode)
-DEF_MACHMODE (V8SImode, "V8SI", MODE_VECTOR_INT, BITS_PER_UNIT*32, 32, 4, V4DImode)
-DEF_MACHMODE (V8DImode, "V8DI", MODE_VECTOR_INT, BITS_PER_UNIT*64, 64, 8, VOIDmode)
+DEF_MACHMODE (V8QImode, "V8QI", MODE_VECTOR_INT, BITS_PER_UNIT*8, 8, 1, V4HImode, QImode)
+DEF_MACHMODE (V8HImode, "V8HI", MODE_VECTOR_INT, BITS_PER_UNIT*16, 16, 2, V4SImode, HImode)
+DEF_MACHMODE (V8SImode, "V8SI", MODE_VECTOR_INT, BITS_PER_UNIT*32, 32, 4, V4DImode, SImode)
+DEF_MACHMODE (V8DImode, "V8DI", MODE_VECTOR_INT, BITS_PER_UNIT*64, 64, 8, VOIDmode, DImode)
 
-DEF_MACHMODE (V16QImode, "V16QI", MODE_VECTOR_INT, BITS_PER_UNIT*16, 16, 1, V8HImode)
+DEF_MACHMODE (V16QImode, "V16QI", MODE_VECTOR_INT, BITS_PER_UNIT*16, 16, 1, V8HImode, QImode)
 
-DEF_MACHMODE (V2SFmode, "V2SF", MODE_VECTOR_FLOAT, BITS_PER_UNIT*8, 8, 4, V4SFmode)
-DEF_MACHMODE (V2DFmode, "V2DF", MODE_VECTOR_FLOAT, BITS_PER_UNIT*16, 16, 8, V8SFmode)
+DEF_MACHMODE (V2SFmode, "V2SF", MODE_VECTOR_FLOAT, BITS_PER_UNIT*8, 8, 4, V4SFmode, SFmode)
+DEF_MACHMODE (V2DFmode, "V2DF", MODE_VECTOR_FLOAT, BITS_PER_UNIT*16, 16, 8, V8SFmode, DFmode)
 
-DEF_MACHMODE (V4SFmode, "V4SF", MODE_VECTOR_FLOAT, BITS_PER_UNIT*16, 16, 4, V2DFmode)
-DEF_MACHMODE (V4DFmode, "V4DF", MODE_VECTOR_FLOAT, BITS_PER_UNIT*32, 32, 8, V8DFmode)
+DEF_MACHMODE (V4SFmode, "V4SF", MODE_VECTOR_FLOAT, BITS_PER_UNIT*16, 16, 4, V2DFmode, SFmode)
+DEF_MACHMODE (V4DFmode, "V4DF", MODE_VECTOR_FLOAT, BITS_PER_UNIT*32, 32, 8, V8DFmode, DFmode)
 
-DEF_MACHMODE (V8SFmode, "V8SF", MODE_VECTOR_FLOAT, BITS_PER_UNIT*32, 32, 4,V4DFmode)
-DEF_MACHMODE (V8DFmode, "V8DF", MODE_VECTOR_FLOAT, BITS_PER_UNIT*64, 64, 8, VOIDmode)
-DEF_MACHMODE (V16SFmode, "V16SF", MODE_VECTOR_FLOAT, 512, 64, 4, VOIDmode)
+DEF_MACHMODE (V8SFmode, "V8SF", MODE_VECTOR_FLOAT, BITS_PER_UNIT*32, 32, 4,V4DFmode, SFmode)
+DEF_MACHMODE (V8DFmode, "V8DF", MODE_VECTOR_FLOAT, BITS_PER_UNIT*64, 64, 8, VOIDmode, DFmode)
+DEF_MACHMODE (V16SFmode, "V16SF", MODE_VECTOR_FLOAT, 512, 64, 4, VOIDmode, SFmode)
 
 /* BLKmode is used for structures, arrays, etc.
    that fit no more specific mode.  */
-DEF_MACHMODE (BLKmode, "BLK", MODE_RANDOM, 0, 0, 0, VOIDmode)
+DEF_MACHMODE (BLKmode, "BLK", MODE_RANDOM, 0, 0, 0, VOIDmode, VOIDmode)
 
 /* The modes for representing the condition codes come last.  CCmode
    is always defined.  Additional modes for the condition code can be
    specified in the EXTRA_CC_MODES macro.  All MODE_CC modes are the
    same width as SImode and have VOIDmode as their next wider mode.  */
 
-#define CC(E, M)  DEF_MACHMODE (E, M, MODE_CC, BITS_PER_UNIT*4, 4, 4, VOIDmode)
+#define CC(E, M)  DEF_MACHMODE (E, M, MODE_CC, BITS_PER_UNIT*4, 4, 4, VOIDmode, VOIDmode)
 
 CC (CCmode, "CC")
 
@@ -167,7 +171,7 @@ EXTRA_CC_MODES
    lot of redundancy in ports that support both 32-bit and 64-bit targets.  */
 #ifdef GENERATOR_FILE
 #undef Pmode
-DEF_MACHMODE (Pmode, "P", MODE_RANDOM, 0, 0, 0, VOIDmode)
+DEF_MACHMODE (Pmode, "P", MODE_RANDOM, 0, 0, 0, VOIDmode, VOIDmode)
 #endif
 
 /*
-- 
cgit v1.1

