/* Definitions of target machine for GNU compiler, for ARM.
   Copyright (C) 2002-2018 Free Software Foundation, Inc.
   Contributed by Pieter `Tiggr' Schoenmakers (rcpieter@win.tue.nl)
   and Martin Simmons (@harleqn.co.uk).
   More major hacks by Richard Earnshaw (rearnsha@arm.com)
   Minor hacks by Nick Clifton (nickc@cygnus.com)

   This file is part of GCC.

   GCC is free software; you can redistribute it and/or modify it
   under the terms of the GNU General Public License as published
   by the Free Software Foundation; either version 3, or (at your
   option) any later version.

   GCC is distributed in the hope that it will be useful, but WITHOUT
   ANY WARRANTY; without even the implied warranty of MERCHANTABILITY
   or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public
   License for more details.

   You should have received a copy of the GNU General Public License
   along with GCC; see the file COPYING3.  If not see
   <http://www.gnu.org/licenses/>.  */


/* Half-precision floating point */
FLOAT_MODE (HF, 2, 0);
ADJUST_FLOAT_FORMAT (HF, ((arm_fp16_format == ARM_FP16_FORMAT_ALTERNATIVE)
			  ? &arm_half_format : &ieee_half_format));

/* CCFPEmode should be used with floating inequalities,
   CCFPmode should be used with floating equalities.
   CC_NOOVmode should be used with SImode integer equalities.
   CC_Zmode should be used if only the Z flag is set correctly
   CC_Cmode should be used if only the C flag is set correctly, after an
     addition.
   CC_Nmode should be used if only the N (sign) flag is set correctly
   CC_CZmode should be used if only the C and Z flags are correct
   (used for DImode unsigned comparisons).
   CC_NCVmode should be used if only the N, C, and V flags are correct
   (used for DImode signed comparisons).
   CCmode should be used otherwise.  */

CC_MODE (CC_NOOV);
CC_MODE (CC_Z);
CC_MODE (CC_CZ);
CC_MODE (CC_NCV);
CC_MODE (CC_SWP);
CC_MODE (CCFP);
CC_MODE (CCFPE);
CC_MODE (CC_DNE);
CC_MODE (CC_DEQ);
CC_MODE (CC_DLE);
CC_MODE (CC_DLT);
CC_MODE (CC_DGE);
CC_MODE (CC_DGT);
CC_MODE (CC_DLEU);
CC_MODE (CC_DLTU);
CC_MODE (CC_DGEU);
CC_MODE (CC_DGTU);
CC_MODE (CC_C);
CC_MODE (CC_N);
CC_MODE (CC_V);

/* Vector modes.  */
VECTOR_MODES (INT, 4);        /*            V4QI V2HI */
VECTOR_MODES (INT, 8);        /*       V8QI V4HI V2SI */
VECTOR_MODES (INT, 16);       /* V16QI V8HI V4SI V2DI */
VECTOR_MODES (FLOAT, 8);      /*            V4HF V2SF */
VECTOR_MODES (FLOAT, 16);     /*       V8HF V4SF V2DF */
VECTOR_MODE (FLOAT, HF, 2);   /*                 V2HF */

/* Fraction and accumulator vector modes.  */
VECTOR_MODES (FRACT, 4);      /* V4QQ  V2HQ */
VECTOR_MODES (UFRACT, 4);     /* V4UQQ V2UHQ */
VECTOR_MODES (ACCUM, 4);      /*       V2HA */
VECTOR_MODES (UACCUM, 4);     /*       V2UHA */

/* Opaque integer modes for 3, 4, 6 or 8 Neon double registers (2 is
   TImode).  */
INT_MODE (EI, 24);
INT_MODE (OI, 32);
INT_MODE (CI, 48);
INT_MODE (XI, 64);
