/* AVR MCUs.
   Copyright (C) 2009, 2010, 2011
   Free Software Foundation, Inc.

   This file is part of GCC.

   GCC is free software; you can redistribute it and/or modify
   it under the terms of the GNU General Public License as published by
   the Free Software Foundation; either version 3, or (at your option)
   any later version.
   
   GCC is distributed in the hope that it will be useful,
   but WITHOUT ANY WARRANTY; without even the implied warranty of
   MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
   GNU General Public License for more details.
   
   You should have received a copy of the GNU General Public License
   along with GCC; see the file COPYING3.  If not see
   <http://www.gnu.org/licenses/>.  */

/* List of all known AVR MCU types - if updated, it has to be kept
   in sync in several places (FIXME: is there a better way?):
    - here;
    - t-avr (MULTILIB_MATCHES);
    - gas/config/tc-avr.c;
    - avr-libc.

   Before including this file, define a macro:

   AVR_MCU (NAME, ARCH, MACRO, SHORT_SP, ERRATA_SKIP, DATA_SEC, LIBRARY_NAME)

   where the arguments are the fields of struct mcu_type_s.  */

/* "avr2" must be first for the "0" default to work as intended.  */

/* Classic, <= 8K.  */
AVR_MCU ("avr2",                 ARCH_AVR2, NULL,                        0, 1, 0x0060, "s8515")
AVR_MCU ("at90s2313",            ARCH_AVR2, "__AVR_AT90S2313__",         1, 0, 0x0060, "s2313")
AVR_MCU ("at90s2323",            ARCH_AVR2, "__AVR_AT90S2323__",         1, 0, 0x0060, "s2323")
AVR_MCU ("at90s2333",            ARCH_AVR2, "__AVR_AT90S2333__",         1, 0, 0x0060, "s2333")
AVR_MCU ("at90s2343",            ARCH_AVR2, "__AVR_AT90S2343__",         1, 0, 0x0060, "s2343")
AVR_MCU ("attiny22",             ARCH_AVR2, "__AVR_ATtiny22__",          1, 0, 0x0060, "tn22")
AVR_MCU ("attiny26",             ARCH_AVR2, "__AVR_ATtiny26__",          1, 0, 0x0060, "tn26")
AVR_MCU ("at90s4414",            ARCH_AVR2, "__AVR_AT90S4414__",         0, 0, 0x0060, "s4414")
AVR_MCU ("at90s4433",            ARCH_AVR2, "__AVR_AT90S4433__",         1, 0, 0x0060, "s4433")
AVR_MCU ("at90s4434",            ARCH_AVR2, "__AVR_AT90S4434__",         0, 0, 0x0060, "s4434")
AVR_MCU ("at90s8515",            ARCH_AVR2, "__AVR_AT90S8515__",         0, 1, 0x0060, "s8515")
AVR_MCU ("at90c8534",            ARCH_AVR2, "__AVR_AT90C8534__",         0, 0, 0x0060, "c8534")
AVR_MCU ("at90s8535",            ARCH_AVR2, "__AVR_AT90S8535__",         0, 0, 0x0060, "s8535")
/* Classic + MOVW, <= 8K.  */
AVR_MCU ("avr25",                ARCH_AVR25, NULL,                       0, 0, 0x0060, "tn85")
AVR_MCU ("ata6289",              ARCH_AVR25, "__AVR_ATA6289__",          0, 0, 0x0100, "a6289")
AVR_MCU ("attiny13",             ARCH_AVR25, "__AVR_ATtiny13__",         1, 0, 0x0060, "tn13")
AVR_MCU ("attiny13a",            ARCH_AVR25, "__AVR_ATtiny13A__",        1, 0, 0x0060, "tn13a")
AVR_MCU ("attiny2313",           ARCH_AVR25, "__AVR_ATtiny2313__",       1, 0, 0x0060, "tn2313")
AVR_MCU ("attiny2313a",          ARCH_AVR25, "__AVR_ATtiny2313A__",      1, 0, 0x0060, "tn2313a")
AVR_MCU ("attiny24",             ARCH_AVR25, "__AVR_ATtiny24__",         1, 0, 0x0060, "tn24")
AVR_MCU ("attiny24a",            ARCH_AVR25, "__AVR_ATtiny24A__",        1, 0, 0x0060, "tn24a")
AVR_MCU ("attiny4313",           ARCH_AVR25, "__AVR_ATtiny4313__",       1, 0, 0x0060, "tn4313")
AVR_MCU ("attiny44",             ARCH_AVR25, "__AVR_ATtiny44__",         0, 0, 0x0060, "tn44")
AVR_MCU ("attiny44a",            ARCH_AVR25, "__AVR_ATtiny44A__",        0, 0, 0x0060, "tn44a")
AVR_MCU ("attiny84",             ARCH_AVR25, "__AVR_ATtiny84__",         0, 0, 0x0060, "tn84")
AVR_MCU ("attiny84a",            ARCH_AVR25, "__AVR_ATtiny84A__",        0, 0, 0x0060, "tn84")
AVR_MCU ("attiny25",             ARCH_AVR25, "__AVR_ATtiny25__",         1, 0, 0x0060, "tn25")
AVR_MCU ("attiny45",             ARCH_AVR25, "__AVR_ATtiny45__",         0, 0, 0x0060, "tn45")
AVR_MCU ("attiny85",             ARCH_AVR25, "__AVR_ATtiny85__",         0, 0, 0x0060, "tn85")
AVR_MCU ("attiny261",            ARCH_AVR25, "__AVR_ATtiny261__",        1, 0, 0x0060, "tn261")
AVR_MCU ("attiny261a",           ARCH_AVR25, "__AVR_ATtiny261A__",       1, 0, 0x0060, "tn261a")
AVR_MCU ("attiny461",            ARCH_AVR25, "__AVR_ATtiny461__",        0, 0, 0x0060, "tn461")
AVR_MCU ("attiny461a",           ARCH_AVR25, "__AVR_ATtiny461A__",       0, 0, 0x0060, "tn461a")
AVR_MCU ("attiny861",            ARCH_AVR25, "__AVR_ATtiny861__",        0, 0, 0x0060, "tn861")
AVR_MCU ("attiny861a",           ARCH_AVR25, "__AVR_ATtiny861A__",       0, 0, 0x0060, "tn861a")
AVR_MCU ("attiny43u",            ARCH_AVR25, "__AVR_ATtiny43U__",        0, 0, 0x0060, "tn43u")
AVR_MCU ("attiny87",             ARCH_AVR25, "__AVR_ATtiny87__",         0, 0, 0x0100, "tn87")
AVR_MCU ("attiny48",             ARCH_AVR25, "__AVR_ATtiny48__",         0, 0, 0x0100, "tn48")
AVR_MCU ("attiny88",             ARCH_AVR25, "__AVR_ATtiny88__",         0, 0, 0x0100, "tn88")
AVR_MCU ("at86rf401",            ARCH_AVR25, "__AVR_AT86RF401__",        1, 0, 0x0060, "86401")
/* Classic, > 8K, <= 64K.  */
AVR_MCU ("avr3",                 ARCH_AVR3, NULL,                        0, 0, 0x0060, "43355")
AVR_MCU ("at43usb355",           ARCH_AVR3, "__AVR_AT43USB355__",        0, 0, 0x0060, "43355")
AVR_MCU ("at76c711",             ARCH_AVR3, "__AVR_AT76C711__",          0, 0, 0x0060, "76711")
/* Classic, == 128K.  */
AVR_MCU ("avr31",                ARCH_AVR31, NULL,                       0, 1, 0x0060, "m103")
AVR_MCU ("atmega103",            ARCH_AVR31, "__AVR_ATmega103__",        0, 1, 0x0060, "m103")
AVR_MCU ("at43usb320",           ARCH_AVR31, "__AVR_AT43USB320__",       0, 0, 0x0060, "43320")
/* Classic + MOVW + JMP/CALL.  */
AVR_MCU ("avr35",                ARCH_AVR35, NULL,                       0, 0, 0x0100, "usb162")
AVR_MCU ("at90usb82",            ARCH_AVR35, "__AVR_AT90USB82__",        0, 0, 0x0100, "usb82")
AVR_MCU ("at90usb162",           ARCH_AVR35, "__AVR_AT90USB162__",       0, 0, 0x0100, "usb162")
AVR_MCU ("atmega8u2",            ARCH_AVR35, "__AVR_ATmega8U2__",        0, 0, 0x0100, "m8u2")
AVR_MCU ("atmega16u2",           ARCH_AVR35, "__AVR_ATmega16U2__",       0, 0, 0x0100, "m16u2")
AVR_MCU ("atmega32u2",           ARCH_AVR35, "__AVR_ATmega32U2__",       0, 0, 0x0100, "m32u2")
AVR_MCU ("attiny167",            ARCH_AVR35, "__AVR_ATtiny167__",        0, 0, 0x0100, "tn167")
/* Enhanced, <= 8K.  */
AVR_MCU ("avr4",                 ARCH_AVR4, NULL,                        0, 0, 0x0060, "m8")
AVR_MCU ("atmega8",              ARCH_AVR4, "__AVR_ATmega8__",           0, 0, 0x0060, "m8")
AVR_MCU ("atmega48",             ARCH_AVR4, "__AVR_ATmega48__",          0, 0, 0x0100, "m48")
AVR_MCU ("atmega48a",            ARCH_AVR4, "__AVR_ATmega48A__",         0, 0, 0x0100, "m48a")
AVR_MCU ("atmega48p",            ARCH_AVR4, "__AVR_ATmega48P__",         0, 0, 0x0100, "m48p")
AVR_MCU ("atmega88",             ARCH_AVR4, "__AVR_ATmega88__",          0, 0, 0x0100, "m88")
AVR_MCU ("atmega88a",            ARCH_AVR4, "__AVR_ATmega88A__",         0, 0, 0x0100, "m88a")
AVR_MCU ("atmega88p",            ARCH_AVR4, "__AVR_ATmega88P__",         0, 0, 0x0100, "m88p")
AVR_MCU ("atmega88pa",           ARCH_AVR4, "__AVR_ATmega88PA__",        0, 0, 0x0100, "m88pa")
AVR_MCU ("atmega8515",           ARCH_AVR4, "__AVR_ATmega8515__",        0, 0, 0x0060, "m8515")
AVR_MCU ("atmega8535",           ARCH_AVR4, "__AVR_ATmega8535__",        0, 0, 0x0060, "m8535")
AVR_MCU ("atmega8hva",           ARCH_AVR4, "__AVR_ATmega8HVA__",        0, 0, 0x0100, "m8hva")
AVR_MCU ("at90pwm1",             ARCH_AVR4, "__AVR_AT90PWM1__",          0, 0, 0x0100, "90pwm1")
AVR_MCU ("at90pwm2",             ARCH_AVR4, "__AVR_AT90PWM2__",          0, 0, 0x0100, "90pwm2")
AVR_MCU ("at90pwm2b",            ARCH_AVR4, "__AVR_AT90PWM2B__",         0, 0, 0x0100, "90pwm2b")
AVR_MCU ("at90pwm3",             ARCH_AVR4, "__AVR_AT90PWM3__",          0, 0, 0x0100, "90pwm3")
AVR_MCU ("at90pwm3b",            ARCH_AVR4, "__AVR_AT90PWM3B__",         0, 0, 0x0100, "90pwm3b")
AVR_MCU ("at90pwm81",            ARCH_AVR4, "__AVR_AT90PWM81__",         0, 0, 0x0100, "90pwm81")
/* Enhanced, > 8K, <= 64K.  */
AVR_MCU ("avr5",                 ARCH_AVR5, NULL,                        0, 0, 0x0060, "m16")
AVR_MCU ("atmega16",             ARCH_AVR5, "__AVR_ATmega16__",          0, 0, 0x0060, "m16")
AVR_MCU ("atmega16a",            ARCH_AVR5, "__AVR_ATmega16A__",         0, 0, 0x0060, "m16a")
AVR_MCU ("atmega161",            ARCH_AVR5, "__AVR_ATmega161__",         0, 0, 0x0060, "m161")
AVR_MCU ("atmega162",            ARCH_AVR5, "__AVR_ATmega162__",         0, 0, 0x0100, "m162")
AVR_MCU ("atmega163",            ARCH_AVR5, "__AVR_ATmega163__",         0, 0, 0x0060, "m163")
AVR_MCU ("atmega164a",           ARCH_AVR5, "__AVR_ATmega164A__",        0, 0, 0x0100, "m164a")
AVR_MCU ("atmega164p",           ARCH_AVR5, "__AVR_ATmega164P__",        0, 0, 0x0100, "m164p")
AVR_MCU ("atmega165",            ARCH_AVR5, "__AVR_ATmega165__",         0, 0, 0x0100, "m165")
AVR_MCU ("atmega165a",           ARCH_AVR5, "__AVR_ATmega165A__",        0, 0, 0x0100, "m165a")
AVR_MCU ("atmega165p",           ARCH_AVR5, "__AVR_ATmega165P__",        0, 0, 0x0100, "m165p")
AVR_MCU ("atmega168",            ARCH_AVR5, "__AVR_ATmega168__",         0, 0, 0x0100, "m168")
AVR_MCU ("atmega168a",           ARCH_AVR5, "__AVR_ATmega168A__",        0, 0, 0x0100, "m168a")
AVR_MCU ("atmega168p",           ARCH_AVR5, "__AVR_ATmega168P__",        0, 0, 0x0100, "m168p")
AVR_MCU ("atmega169",            ARCH_AVR5, "__AVR_ATmega169__",         0, 0, 0x0100, "m169")
AVR_MCU ("atmega169a",           ARCH_AVR5, "__AVR_ATmega169A__",        0, 0, 0x0100, "m169a")
AVR_MCU ("atmega169p",           ARCH_AVR5, "__AVR_ATmega169P__",        0, 0, 0x0100, "m169p")
AVR_MCU ("atmega169pa",          ARCH_AVR5, "__AVR_ATmega169PA__",       0, 0, 0x0100, "m169pa")
AVR_MCU ("atmega32",             ARCH_AVR5, "__AVR_ATmega32__",          0, 0, 0x0060, "m32")
AVR_MCU ("atmega323",            ARCH_AVR5, "__AVR_ATmega323__",         0, 0, 0x0060, "m323")
AVR_MCU ("atmega324a",           ARCH_AVR5, "__AVR_ATmega324A__",        0, 0, 0x0100, "m324a")
AVR_MCU ("atmega324p",           ARCH_AVR5, "__AVR_ATmega324P__",        0, 0, 0x0100, "m324p")
AVR_MCU ("atmega324pa",          ARCH_AVR5, "__AVR_ATmega324PA__",       0, 0, 0x0100, "m324pa")
AVR_MCU ("atmega325",            ARCH_AVR5, "__AVR_ATmega325__",         0, 0, 0x0100, "m325")
AVR_MCU ("atmega325a",           ARCH_AVR5, "__AVR_ATmega325A__",        0, 0, 0x0100, "m325a")
AVR_MCU ("atmega325p",           ARCH_AVR5, "__AVR_ATmega325P__",        0, 0, 0x0100, "m325p")
AVR_MCU ("atmega3250",           ARCH_AVR5, "__AVR_ATmega3250__",        0, 0, 0x0100, "m3250")
AVR_MCU ("atmega3250a",          ARCH_AVR5, "__AVR_ATmega3250A__",       0, 0, 0x0100, "m3250a")
AVR_MCU ("atmega3250p",          ARCH_AVR5, "__AVR_ATmega3250P__",       0, 0, 0x0100, "m3250p")
AVR_MCU ("atmega328",            ARCH_AVR5, "__AVR_ATmega328__",         0, 0, 0x0100, "m328")
AVR_MCU ("atmega328p",           ARCH_AVR5, "__AVR_ATmega328P__",        0, 0, 0x0100, "m328p")
AVR_MCU ("atmega329",            ARCH_AVR5, "__AVR_ATmega329__",         0, 0, 0x0100, "m329")
AVR_MCU ("atmega329a",           ARCH_AVR5, "__AVR_ATmega329A__",        0, 0, 0x0100, "m329a")
AVR_MCU ("atmega329p",           ARCH_AVR5, "__AVR_ATmega329P__",        0, 0, 0x0100, "m329p")
AVR_MCU ("atmega329pa",          ARCH_AVR5, "__AVR_ATmega329PA__",       0, 0, 0x0100, "m329pa")
AVR_MCU ("atmega3290",           ARCH_AVR5, "__AVR_ATmega3290__",        0, 0, 0x0100, "m3290")
AVR_MCU ("atmega3290a",          ARCH_AVR5, "__AVR_ATmega3290A__",       0, 0, 0x0100, "m3290a")
AVR_MCU ("atmega3290p",          ARCH_AVR5, "__AVR_ATmega3290P__",       0, 0, 0x0100, "m3290p")
AVR_MCU ("atmega406",            ARCH_AVR5, "__AVR_ATmega406__",         0, 0, 0x0100, "m406")
AVR_MCU ("atmega64",             ARCH_AVR5, "__AVR_ATmega64__",          0, 0, 0x0100, "m64")
AVR_MCU ("atmega640",            ARCH_AVR5, "__AVR_ATmega640__",         0, 0, 0x0200, "m640")
AVR_MCU ("atmega644",            ARCH_AVR5, "__AVR_ATmega644__",         0, 0, 0x0100, "m644")
AVR_MCU ("atmega644a",           ARCH_AVR5, "__AVR_ATmega644A__",        0, 0, 0x0100, "m644a")
AVR_MCU ("atmega644p",           ARCH_AVR5, "__AVR_ATmega644P__",        0, 0, 0x0100, "m644p")
AVR_MCU ("atmega644pa",          ARCH_AVR5, "__AVR_ATmega644PA__",       0, 0, 0x0100, "m644pa")
AVR_MCU ("atmega645",            ARCH_AVR5, "__AVR_ATmega645__",         0, 0, 0x0100, "m645")
AVR_MCU ("atmega645a",           ARCH_AVR5, "__AVR_ATmega645A__",        0, 0, 0x0100, "m645a")
AVR_MCU ("atmega645p",           ARCH_AVR5, "__AVR_ATmega645P__",        0, 0, 0x0100, "m645p")
AVR_MCU ("atmega6450",           ARCH_AVR5, "__AVR_ATmega6450__",        0, 0, 0x0100, "m6450")
AVR_MCU ("atmega6450a",          ARCH_AVR5, "__AVR_ATmega6450A__",       0, 0, 0x0100, "m6450a")
AVR_MCU ("atmega6450p",          ARCH_AVR5, "__AVR_ATmega6450P__",       0, 0, 0x0100, "m6450p")
AVR_MCU ("atmega649",            ARCH_AVR5, "__AVR_ATmega649__",         0, 0, 0x0100, "m649")
AVR_MCU ("atmega649a",           ARCH_AVR5, "__AVR_ATmega649A__",        0, 0, 0x0100, "m649a")
AVR_MCU ("atmega649p",           ARCH_AVR5, "__AVR_ATmega649P__",        0, 0, 0x0100, "m649p")
AVR_MCU ("atmega6490",           ARCH_AVR5, "__AVR_ATmega6490__",        0, 0, 0x0100, "m6490")
AVR_MCU ("atmega16hva",          ARCH_AVR5, "__AVR_ATmega16HVA__",       0, 0, 0x0100, "m16hva")
AVR_MCU ("atmega16hva2",         ARCH_AVR5, "__AVR_ATmega16HVA2__",      0, 0, 0x0100, "m16hva2")
AVR_MCU ("atmega16hvb",          ARCH_AVR5, "__AVR_ATmega16HVB__",       0, 0, 0x0100, "m16hvb")
AVR_MCU ("atmega32hvb",          ARCH_AVR5, "__AVR_ATmega32HVB__",       0, 0, 0x0100, "m32hvb")
AVR_MCU ("atmega64hve",          ARCH_AVR5, "__AVR_ATmega64HVE__",       0, 0, 0x0100, "m64hve")
AVR_MCU ("at90can32",            ARCH_AVR5, "__AVR_AT90CAN32__",         0, 0, 0x0100, "can32")
AVR_MCU ("at90can64",            ARCH_AVR5, "__AVR_AT90CAN64__",         0, 0, 0x0100, "can64")
AVR_MCU ("at90pwm216",           ARCH_AVR5, "__AVR_AT90PWM216__",        0, 0, 0x0100, "90pwm216")
AVR_MCU ("at90pwm316",           ARCH_AVR5, "__AVR_AT90PWM316__",        0, 0, 0x0100, "90pwm316")
AVR_MCU ("atmega32c1",           ARCH_AVR5, "__AVR_ATmega32C1__",        0, 0, 0x0100, "m32c1")
AVR_MCU ("atmega64c1",           ARCH_AVR5, "__AVR_ATmega64C1__",        0, 0, 0x0100, "m64c1")
AVR_MCU ("atmega16m1",           ARCH_AVR5, "__AVR_ATmega16M1__",        0, 0, 0x0100, "m16m1")
AVR_MCU ("atmega32m1",           ARCH_AVR5, "__AVR_ATmega32M1__",        0, 0, 0x0100, "m32m1")
AVR_MCU ("atmega64m1",           ARCH_AVR5, "__AVR_ATmega64M1__",        0, 0, 0x0100, "m64m1")
AVR_MCU ("atmega16u4",           ARCH_AVR5, "__AVR_ATmega16U4__",        0, 0, 0x0100, "m16u4")
AVR_MCU ("atmega32u4",           ARCH_AVR5, "__AVR_ATmega32U4__",        0, 0, 0x0100, "m32u4")
AVR_MCU ("atmega32u6",           ARCH_AVR5, "__AVR_ATmega32U6__",        0, 0, 0x0100, "m32u6")
AVR_MCU ("at90scr100",           ARCH_AVR5, "__AVR_AT90SCR100__",        0, 0, 0x0100, "90scr100")
AVR_MCU ("at90usb646",           ARCH_AVR5, "__AVR_AT90USB646__",        0, 0, 0x0100, "usb646")
AVR_MCU ("at90usb647",           ARCH_AVR5, "__AVR_AT90USB647__",        0, 0, 0x0100, "usb647")
AVR_MCU ("at94k",                ARCH_AVR5, "__AVR_AT94K__",             0, 0, 0x0060, "at94k")
AVR_MCU ("m3000",                ARCH_AVR5, "__AVR_M3000__",             0, 0, 0x1000, "m3000")
/* Enhanced, == 128K.  */
AVR_MCU ("avr51",                ARCH_AVR51, NULL,                       0, 0, 0x0100, "m128")
AVR_MCU ("atmega128",            ARCH_AVR51, "__AVR_ATmega128__",        0, 0, 0x0100, "m128")
AVR_MCU ("atmega1280",           ARCH_AVR51, "__AVR_ATmega1280__",       0, 0, 0x0200, "m1280")
AVR_MCU ("atmega1281",           ARCH_AVR51, "__AVR_ATmega1281__",       0, 0, 0x0200, "m1281")
AVR_MCU ("atmega1284p",          ARCH_AVR51, "__AVR_ATmega1284P__",      0, 0, 0x0100, "m1284p")
AVR_MCU ("atmega128rfa1",        ARCH_AVR51, "__AVR_ATmega128RFA1__",    0, 0, 0x0200, "m128rfa1")
AVR_MCU ("at90can128",           ARCH_AVR51, "__AVR_AT90CAN128__",       0, 0, 0x0100, "can128")
AVR_MCU ("at90usb1286",          ARCH_AVR51, "__AVR_AT90USB1286__",      0, 0, 0x0100, "usb1286")
AVR_MCU ("at90usb1287",          ARCH_AVR51, "__AVR_AT90USB1287__",      0, 0, 0x0100, "usb1286")
/* 3-Byte PC.  */
AVR_MCU ("avr6",                 ARCH_AVR6, NULL,                        0, 0, 0x0200, "m2561")
AVR_MCU ("atmega2560",           ARCH_AVR6, "__AVR_ATmega2560__",        0, 0, 0x0200, "m2560")
AVR_MCU ("atmega2561",           ARCH_AVR6, "__AVR_ATmega2561__",        0, 0, 0x0200, "m2561")
/* Assembler only.  */
AVR_MCU ("avr1",                 ARCH_AVR1, NULL,                        0, 0, 0x0060, "s1200")
AVR_MCU ("at90s1200",            ARCH_AVR1, "__AVR_AT90S1200__",         0, 0, 0x0060, "s1200")
AVR_MCU ("attiny11",             ARCH_AVR1, "__AVR_ATtiny11__",          0, 0, 0x0060, "tn11")
AVR_MCU ("attiny12",             ARCH_AVR1, "__AVR_ATtiny12__",          0, 0, 0x0060, "tn12")
AVR_MCU ("attiny15",             ARCH_AVR1, "__AVR_ATtiny15__",          0, 0, 0x0060, "tn15")
AVR_MCU ("attiny28",             ARCH_AVR1, "__AVR_ATtiny28__",          0, 0, 0x0060, "tn28")
