FRACTIONAL_INT_MODE (PSI, 24, 3);
