/* 20-bit address */
PARTIAL_INT_MODE (SI);

