/* 20-bit address */
PARTIAL_INT_MODE (SI, 20, PSI);

