/* IBM RS/6000 CPU names..
   Copyright (C) 1991, 1993, 1994, 1995, 1996, 1997, 1998, 1999,
   2000, 2001, 2002, 2003, 2004, 2005, 2006, 2007, 2008, 2009, 2010, 2011
   Free Software Foundation, Inc.
   Contributed by Richard Kenner (kenner@vlsi1.ultra.nyu.edu)

   This file is part of GCC.

   GCC is free software; you can redistribute it and/or modify it
   under the terms of the GNU General Public License as published
   by the Free Software Foundation; either version 3, or (at your
   option) any later version.

   GCC is distributed in the hope that it will be useful, but WITHOUT
   ANY WARRANTY; without even the implied warranty of MERCHANTABILITY
   or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public
   License for more details.

   You should have received a copy of the GNU General Public License
   along with GCC; see the file COPYING3.  If not see
   <http://www.gnu.org/licenses/>.  */

/* This table occasionally claims that a processor does not support a
   particular feature even though it does, but the feature is slower than the
   alternative.  Thus, it shouldn't be relied on as a complete description of
   the processor's support.

   Please keep this list in order, and don't forget to update the documentation
   in invoke.texi when adding a new processor or flag.

   Before including this file, define a macro:

   RS6000_CPU (NAME, CPU, FLAGS)

   where the arguments are the fields of struct rs6000_ptt.  */

RS6000_CPU ("401", PROCESSOR_PPC403, POWERPC_BASE_MASK | MASK_SOFT_FLOAT)
RS6000_CPU ("403", PROCESSOR_PPC403,
	    POWERPC_BASE_MASK | MASK_SOFT_FLOAT | MASK_STRICT_ALIGN)
RS6000_CPU ("405", PROCESSOR_PPC405,
	    POWERPC_BASE_MASK | MASK_SOFT_FLOAT | MASK_MULHW | MASK_DLMZB)
RS6000_CPU ("405fp", PROCESSOR_PPC405,
	    POWERPC_BASE_MASK | MASK_MULHW | MASK_DLMZB)
RS6000_CPU ("440", PROCESSOR_PPC440,
	    POWERPC_BASE_MASK | MASK_SOFT_FLOAT | MASK_MULHW | MASK_DLMZB)
RS6000_CPU ("440fp", PROCESSOR_PPC440,
	    POWERPC_BASE_MASK | MASK_MULHW | MASK_DLMZB)
RS6000_CPU ("464", PROCESSOR_PPC440,
	    POWERPC_BASE_MASK | MASK_SOFT_FLOAT | MASK_MULHW | MASK_DLMZB)
RS6000_CPU ("464fp", PROCESSOR_PPC440,
	    POWERPC_BASE_MASK | MASK_MULHW | MASK_DLMZB)
RS6000_CPU ("476", PROCESSOR_PPC476,
	    POWERPC_BASE_MASK | MASK_SOFT_FLOAT | MASK_PPC_GFXOPT | MASK_MFCRF
	    | MASK_POPCNTB | MASK_FPRND | MASK_CMPB | MASK_MULHW | MASK_DLMZB)
RS6000_CPU ("476fp", PROCESSOR_PPC476,
	    POWERPC_BASE_MASK | MASK_PPC_GFXOPT | MASK_MFCRF | MASK_POPCNTB
	    | MASK_FPRND | MASK_CMPB | MASK_MULHW | MASK_DLMZB)
RS6000_CPU ("505", PROCESSOR_MPCCORE, POWERPC_BASE_MASK)
RS6000_CPU ("601", PROCESSOR_PPC601,
	    MASK_POWER | POWERPC_BASE_MASK | MASK_MULTIPLE | MASK_STRING)
RS6000_CPU ("602", PROCESSOR_PPC603, POWERPC_BASE_MASK | MASK_PPC_GFXOPT)
RS6000_CPU ("603", PROCESSOR_PPC603, POWERPC_BASE_MASK | MASK_PPC_GFXOPT)
RS6000_CPU ("603e", PROCESSOR_PPC603, POWERPC_BASE_MASK | MASK_PPC_GFXOPT)
RS6000_CPU ("604", PROCESSOR_PPC604, POWERPC_BASE_MASK | MASK_PPC_GFXOPT)
RS6000_CPU ("604e", PROCESSOR_PPC604e, POWERPC_BASE_MASK | MASK_PPC_GFXOPT)
RS6000_CPU ("620", PROCESSOR_PPC620,
	    POWERPC_BASE_MASK | MASK_PPC_GFXOPT | MASK_POWERPC64)
RS6000_CPU ("630", PROCESSOR_PPC630,
	    POWERPC_BASE_MASK | MASK_PPC_GFXOPT | MASK_POWERPC64)
RS6000_CPU ("740", PROCESSOR_PPC750, POWERPC_BASE_MASK | MASK_PPC_GFXOPT)
RS6000_CPU ("7400", PROCESSOR_PPC7400, POWERPC_7400_MASK)
RS6000_CPU ("7450", PROCESSOR_PPC7450, POWERPC_7400_MASK)
RS6000_CPU ("750", PROCESSOR_PPC750, POWERPC_BASE_MASK | MASK_PPC_GFXOPT)
RS6000_CPU ("801", PROCESSOR_MPCCORE, POWERPC_BASE_MASK | MASK_SOFT_FLOAT)
RS6000_CPU ("821", PROCESSOR_MPCCORE, POWERPC_BASE_MASK | MASK_SOFT_FLOAT)
RS6000_CPU ("823", PROCESSOR_MPCCORE, POWERPC_BASE_MASK | MASK_SOFT_FLOAT)
RS6000_CPU ("8540", PROCESSOR_PPC8540, POWERPC_BASE_MASK | MASK_STRICT_ALIGN
	    | MASK_ISEL)
/* 8548 has a dummy entry for now.  */
RS6000_CPU ("8548", PROCESSOR_PPC8540, POWERPC_BASE_MASK | MASK_STRICT_ALIGN
	    | MASK_ISEL)
RS6000_CPU ("a2", PROCESSOR_PPCA2,
	    POWERPC_BASE_MASK | MASK_PPC_GFXOPT | MASK_POWERPC64 | MASK_POPCNTB
	    | MASK_CMPB | MASK_NO_UPDATE)
RS6000_CPU ("e300c2", PROCESSOR_PPCE300C2, POWERPC_BASE_MASK | MASK_SOFT_FLOAT)
RS6000_CPU ("e300c3", PROCESSOR_PPCE300C3, POWERPC_BASE_MASK)
RS6000_CPU ("e500mc", PROCESSOR_PPCE500MC, POWERPC_BASE_MASK | MASK_PPC_GFXOPT
	    | MASK_ISEL)
RS6000_CPU ("e500mc64", PROCESSOR_PPCE500MC64,
	    POWERPC_BASE_MASK | MASK_POWERPC64 | MASK_PPC_GFXOPT | MASK_ISEL)
RS6000_CPU ("860", PROCESSOR_MPCCORE, POWERPC_BASE_MASK | MASK_SOFT_FLOAT)
RS6000_CPU ("970", PROCESSOR_POWER4,
	    POWERPC_7400_MASK | MASK_PPC_GPOPT | MASK_MFCRF | MASK_POWERPC64)
RS6000_CPU ("cell", PROCESSOR_CELL,
	    POWERPC_7400_MASK  | MASK_PPC_GPOPT | MASK_MFCRF | MASK_POWERPC64)
RS6000_CPU ("common", PROCESSOR_COMMON, MASK_NEW_MNEMONICS)
RS6000_CPU ("ec603e", PROCESSOR_PPC603, POWERPC_BASE_MASK | MASK_SOFT_FLOAT)
RS6000_CPU ("G3", PROCESSOR_PPC750, POWERPC_BASE_MASK | MASK_PPC_GFXOPT)
RS6000_CPU ("G4",  PROCESSOR_PPC7450, POWERPC_7400_MASK)
RS6000_CPU ("G5", PROCESSOR_POWER4,
	    POWERPC_7400_MASK | MASK_PPC_GPOPT | MASK_MFCRF | MASK_POWERPC64)
RS6000_CPU ("titan", PROCESSOR_TITAN,
	    POWERPC_BASE_MASK | MASK_MULHW | MASK_DLMZB)
RS6000_CPU ("power", PROCESSOR_POWER, MASK_POWER | MASK_MULTIPLE | MASK_STRING)
RS6000_CPU ("power2", PROCESSOR_POWER,
	    MASK_POWER | MASK_POWER2 | MASK_MULTIPLE | MASK_STRING)
RS6000_CPU ("power3", PROCESSOR_PPC630,
	    POWERPC_BASE_MASK | MASK_PPC_GFXOPT | MASK_POWERPC64)
RS6000_CPU ("power4", PROCESSOR_POWER4,
	    POWERPC_BASE_MASK | MASK_POWERPC64 | MASK_PPC_GPOPT
	    | MASK_PPC_GFXOPT | MASK_MFCRF)
RS6000_CPU ("power5", PROCESSOR_POWER5,
	    POWERPC_BASE_MASK | MASK_POWERPC64 | MASK_PPC_GPOPT
	    | MASK_PPC_GFXOPT | MASK_MFCRF | MASK_POPCNTB)
RS6000_CPU ("power5+", PROCESSOR_POWER5,
	    POWERPC_BASE_MASK | MASK_POWERPC64 | MASK_PPC_GPOPT
	    | MASK_PPC_GFXOPT | MASK_MFCRF | MASK_POPCNTB | MASK_FPRND)
RS6000_CPU ("power6", PROCESSOR_POWER6,
	    POWERPC_BASE_MASK | MASK_POWERPC64 | MASK_PPC_GPOPT
	    | MASK_PPC_GFXOPT | MASK_MFCRF | MASK_POPCNTB | MASK_FPRND
	    | MASK_CMPB | MASK_DFP | MASK_RECIP_PRECISION)
RS6000_CPU ("power6x", PROCESSOR_POWER6,
	    POWERPC_BASE_MASK | MASK_POWERPC64 | MASK_PPC_GPOPT
	    | MASK_PPC_GFXOPT | MASK_MFCRF | MASK_POPCNTB | MASK_FPRND
	    | MASK_CMPB | MASK_DFP | MASK_MFPGPR | MASK_RECIP_PRECISION)
RS6000_CPU ("power7", PROCESSOR_POWER7,   /* Don't add MASK_ISEL by default */
	    POWERPC_7400_MASK | MASK_POWERPC64 | MASK_PPC_GPOPT | MASK_MFCRF
	    | MASK_POPCNTB | MASK_FPRND | MASK_CMPB | MASK_DFP | MASK_POPCNTD
	    | MASK_VSX | MASK_RECIP_PRECISION)
RS6000_CPU ("powerpc", PROCESSOR_POWERPC, POWERPC_BASE_MASK)
RS6000_CPU ("powerpc64", PROCESSOR_POWERPC64,
	    POWERPC_BASE_MASK | MASK_PPC_GFXOPT | MASK_POWERPC64)
RS6000_CPU ("rios", PROCESSOR_RIOS1, MASK_POWER | MASK_MULTIPLE | MASK_STRING)
RS6000_CPU ("rios1", PROCESSOR_RIOS1, MASK_POWER | MASK_MULTIPLE | MASK_STRING)
RS6000_CPU ("rios2", PROCESSOR_RIOS2,
	    MASK_POWER | MASK_POWER2 | MASK_MULTIPLE | MASK_STRING)
RS6000_CPU ("rsc", PROCESSOR_PPC601, MASK_POWER | MASK_MULTIPLE | MASK_STRING)
RS6000_CPU ("rsc1", PROCESSOR_PPC601, MASK_POWER | MASK_MULTIPLE | MASK_STRING)
RS6000_CPU ("rs64", PROCESSOR_RS64A,
	    POWERPC_BASE_MASK | MASK_PPC_GFXOPT | MASK_POWERPC64)
