From 80636611f3a1490d8164509f1b206d009d153b61 Mon Sep 17 00:00:00 2001
From: Michael Meissner <meissner@linux.vnet.ibm.com>
Date: Wed, 23 Mar 2016 20:33:28 +0000
Subject: re PR target/70381 (On powerpc, -mfloat128 is on by default for all
 VSX systems)

2016-03-23  Michael Meissner  <meissner@linux.vnet.ibm.com>

	PR target/70381
	* config/rs6000/rs6000-cpus.def (ISA_2_6_MASKS_SERVER): Do not set
	-mfloat128 here.

From-SVN: r234441
---
 gcc/config/rs6000/rs6000-cpus.def | 1 -
 1 file changed, 1 deletion(-)

(limited to 'gcc/config/rs6000/rs6000-cpus.def')

diff --git a/gcc/config/rs6000/rs6000-cpus.def b/gcc/config/rs6000/rs6000-cpus.def
index 92fb71a..275404a 100644
--- a/gcc/config/rs6000/rs6000-cpus.def
+++ b/gcc/config/rs6000/rs6000-cpus.def
@@ -44,7 +44,6 @@
 #define ISA_2_6_MASKS_SERVER	(ISA_2_5_MASKS_SERVER			\
 				 | OPTION_MASK_POPCNTD			\
 				 | OPTION_MASK_ALTIVEC			\
-				 | OPTION_MASK_FLOAT128			\
 				 | OPTION_MASK_VSX			\
 				 | OPTION_MASK_UPPER_REGS_DF)
 
-- 
cgit v1.1

