From 5a59bc1de21921996545574822e92004629dbd37 Mon Sep 17 00:00:00 2001
From: David Hildenbrand <david@redhat.com>
Date: Fri, 8 Dec 2017 17:01:58 +0100
Subject: s390x/tcg: wire up STORE CHANNEL REPORT WORD

CRW machine check handling requires STCRW. So let's wire it up.

Reviewed-by: Thomas Huth <thuth@redhat.com>
Reviewed-by: Richard Henderson <richard.henderson@linaro.org>
Signed-off-by: David Hildenbrand <david@redhat.com>
Message-Id: <20171208160207.26494-6-david@redhat.com>
Signed-off-by: Cornelia Huck <cohuck@redhat.com>
---
 target/s390x/insn-data.def | 1 +
 1 file changed, 1 insertion(+)

(limited to 'target/s390x/insn-data.def')

diff --git a/target/s390x/insn-data.def b/target/s390x/insn-data.def
index 8c2541f..43ab196 100644
--- a/target/s390x/insn-data.def
+++ b/target/s390x/insn-data.def
@@ -1055,6 +1055,7 @@
     C(0xb23b, RCHP,    S,     Z,   0, 0, 0, 0, rchp, 0)
     C(0xb238, RSCH,    S,     Z,   0, 0, 0, 0, rsch, 0)
     C(0xb233, SSCH,    S,     Z,   0, insn, 0, 0, ssch, 0)
+    C(0xb239, STCRW,   S,     Z,   0, insn, 0, 0, stcrw, 0)
     C(0xb234, STSCH,   S,     Z,   0, insn, 0, 0, stsch, 0)
     C(0xb235, TSCH,    S,     Z,   0, insn, 0, 0, tsch, 0)
     /* ??? Not listed in PoO ninth edition, but there's a linux driver that
-- 
cgit v1.1

