From 5ca937811c13ae142f783e69f61f6a402694ebe0 Mon Sep 17 00:00:00 2001
From: Andrew Waterman <andrew@sifive.com>
Date: Tue, 23 Feb 2021 16:47:47 -0800
Subject: s/NSE/Custom/ in RVC spec

Resolves #629
---
 src/c.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'src/c.tex')

diff --git a/src/c.tex b/src/c.tex
index 8799bc4..0a26877 100644
--- a/src/c.tex
+++ b/src/c.tex
@@ -1255,7 +1255,7 @@ least-significant bits set, corresponds to instructions wider
 than 16 bits, including those in the base ISAs.  Several instructions
 are only valid for certain operands; when invalid, they are marked
 either {\em RES} to indicate that the opcode is reserved for future
-standard extensions; {\em NSE} to indicate that the opcode is designated
+standard extensions; {\em Custom} to indicate that the opcode is designated
 for custom extensions; or {\em HINT} to indicate that the opcode
 is reserved for microarchitectural hints (see Section~\ref{sec:rvc-hints}).
 
-- 
cgit v1.1

