From 5e42ce2bd9caf8d907520075a8e9dc564c1f4d30 Mon Sep 17 00:00:00 2001
From: Krste Asanovic <krste@eecs.berkeley.edu>
Date: Mon, 13 Feb 2017 08:00:25 -0800
Subject: Clarified instruction misaligned exceptions on JAL/JALR.

---
 src/c.tex | 6 +++++-
 1 file changed, 5 insertions(+), 1 deletion(-)

(limited to 'src/c.tex')

diff --git a/src/c.tex b/src/c.tex
index 2c81f7b..309689b 100644
--- a/src/c.tex
+++ b/src/c.tex
@@ -34,7 +34,11 @@ versions of common 32-bit RISC-V instructions when:
 The C extension is compatible with all other standard instruction
 extensions.  The C extension allows 16-bit instructions to be freely
 intermixed with 32-bit instructions, with the latter now able to start
-on any 16-bit boundary.
+on any 16-bit boundary.  With the addition of the C extension, JAL and
+JALR instructions will no longer raise an instruction misaligned
+exception.
+
+\pagebreak
 
 \begin{commentary}
 Removing the 32-bit alignment constraint on the original 32-bit
-- 
cgit v1.1

