From a4ade78dcbb56a84d6577b167443fbca3bf82770 Mon Sep 17 00:00:00 2001
From: Andrew Waterman <andrew@sifive.com>
Date: Thu, 22 Feb 2018 01:20:51 -0800
Subject: Introduce IALIGN; propose misa.C semantics

---
 src/c.tex | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

(limited to 'src/c.tex')

diff --git a/src/c.tex b/src/c.tex
index 066c5ef..d13e27c 100644
--- a/src/c.tex
+++ b/src/c.tex
@@ -28,9 +28,9 @@ versions of common 32-bit RISC-V instructions when:
 The C extension is compatible with all other standard instruction
 extensions.  The C extension allows 16-bit instructions to be freely
 intermixed with 32-bit instructions, with the latter now able to start
-on any 16-bit boundary.  With the addition of the C extension, JAL and
-JALR instructions will no longer raise an instruction misaligned
-exception.
+on any 16-bit boundary, i.e., IALIGN=16.  With the addition of the C
+extension, no instructions can raise instruction-address-misaligned
+exceptions.
 
 \pagebreak
 
-- 
cgit v1.1

