From 76f3c072674a3a3b0eeefe767ca1b52107998c8d Mon Sep 17 00:00:00 2001
From: Krste Asanovic <krste@eecs.berkeley.edu>
Date: Mon, 20 Mar 2017 04:10:17 -0700
Subject: Removed explicit convention on shadow CSRs.

---
 src/plic.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'src/plic.tex')

diff --git a/src/plic.tex b/src/plic.tex
index 3319506..fcf366d 100644
--- a/src/plic.tex
+++ b/src/plic.tex
@@ -99,7 +99,7 @@ support delegating external interrupts to lower-privilege modes, then
 the lower-privilege hart contexts will not be interrupt targets.
 Interrupt notifications generated by the PLIC appear in the {\tt
   meip}/{\tt seip}/{\tt ueip} bits of the {\tt mip}/{\tt sip}/{\tt
-  uip} registers for M/H/S/U modes respectively.  The notifications
+  uip} registers for M/S/U modes respectively.  The notifications
 only appear in lower-privilege {\em x}{\tt ip} registers if external
 interrupts have been delegated to the lower-privilege modes.
 
-- 
cgit v1.1

