From 825c9395021ad25ae0726afa91a9a4f27daec2dc Mon Sep 17 00:00:00 2001
From: Andrew Waterman <andrew@sifive.com>
Date: Mon, 25 Mar 2019 01:46:28 -0700
Subject: Change "pc" to "address" for clarity

Resolves #356
---
 src/rv64.tex | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

(limited to 'src/rv64.tex')

diff --git a/src/rv64.tex b/src/rv64.tex
index ef51e62..bde375c 100644
--- a/src/rv64.tex
+++ b/src/rv64.tex
@@ -139,11 +139,11 @@ places zero in the lowest 12 bits.  The 32-bit result is
 sign-extended to 64 bits.
 
 AUIPC (add upper immediate to {\tt pc}) uses the same opcode as RV32I.
-AUIPC (add upper immediate to {\tt pc}) is used to build {\tt
+AUIPC is used to build {\tt
   pc}-relative addresses and uses the U-type format.  AUIPC appends 12
 low-order zero bits to the 20-bit U-immediate, sign-extends the result
-to 64 bits, then adds it to the {\tt pc} and places the result in
-register {\em rd}.
+to 64 bits, adds it to the address of the AUIPC instruction,
+then places the result in register {\em rd}.
 
 \subsubsection*{Integer Register-Register Operations}
 
-- 
cgit v1.1

